Commands for linux:

Cd /media -> to find the usb when plugged in to the coral board

Cd /home/mendel -> ls -> shows where it saved our recording from the board

AudioPlayer(“./recorded/wav”).play(block=True) -> to play audio with headphones plugged in to coral board

<https://stackoverflow.com/questions/66401752/how-to-get-sound-from-pdm-microphone-on-google-coral-dev-board-mini>

Link for code used to record audio on google coral board

MAKE SURE BOARD IS CONNECTED TO INTERNET!!!!!!!

Nmtui -> to get to the networks and choose

Nmcli -> show connections that we are connected to (network)

Log in to laptop

Power up board to wall and connect usb to (LEFT SIDE) of toshiba

“Mdt shell” to log into king dog

“python 3 test.py” to run our code

Cd /home/Mendel

Ls to see all files in this directory

Python3 to get into python terminal

From audioplayer import AudioPlayer

AudioPlayer(“./recorded/wav”).play(block=True) -> to play audio through the board in headphone jack